| Revolve Panel Quick Help |
|  | Quick Help Home nPower Software Home |
| Revolve Paramaters |
| The Pwr_Revolve command creates a solid or surfaces by rotating a profile about a rotation axis. This is similar to the 3ds max "Lathe" command except that it produces a smooth surface instead of polygons. Degrees: Determines the angle of rotation for the revolution. |
| Cap Ends |
| Cap Ends If Closed: Selecting this option will close off the ends of the revolution and make it a closed solid. Turning this option off will leave "holes" in the ends of the revolution. |
| Direction Options |
| Swap Axis XY: changes the rotation axis. Will rotate the profile in the opposite direction. Swap Axis Side: changes the side of the rotation axis that the profile will be rotated about. Similar to a mirror operation. |
| Profile Operations |
| Same as Power Extrude |