| Join Quick Help |
|  | Quick Help Home nPower Software Home |
| Conversion Parameters |
| Power Join provides the ability to join together separate objects into a single NURBS Brep. The following options determine how the objects are combined. Sew Edges To Edges: This option will sew together edges of adjoining surfaces (removing the seams or gaps), making them into a single surface Glue Edges To Surfaces: This option is similar to the "Sew Edges" option except that the surfaces remain separate. Do Nothing: No sewing or merging will be performed Intersect + Merge Faces: Surfaces are intersected and merged together to form a solid object bounded by the merged surfaces |
| Remove Excess Faces |
| Remove Excess Faces: Removes trimmed faces that are outside of the Power NURBS Brep that is being created. For example, surfaces that are merged together (with the "Intersect + Merge Faces" option) will be trimmed back, and the excess material (faces that are outside of the boundary of the resulting solid) will be removed. |